* “Opening Gap” message must be shown as soon as the camera detects the lights and not after some seconds after detecting the vehicle.(R)
* “Happy Journey” message must be shown if there is no gap.(R)